
Computer
********


Summary
-------

-Computer-
Processor		: 8x Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz
Memory		: 6017MB (3363MB used)
Operating System		: Linux Mint 18 Sarah
User Name		: jp (jp)
Date/Time		: sam. 27 août 2016 22:02:25 CEST
-Display-
Resolution		: 2944x1080 pixels
OpenGL Renderer		: Mesa DRI Intel(R) Sandybridge Mobile 
X11 Vendor		: The X.Org Foundation
-Multimedia-
Audio Adapter		: HDA-Intel - HDA Intel PCH
-Input Devices-
 Lid Switch
 Sleep Button
 Power Button
 AT Translated Set 2 keyboard
 Video Bus
 Video Bus
 ETPS/2 Elantech Touchpad
 USB2.0 UVC 2M WebCam
 Asus WMI hotkeys
 HDA Intel PCH Mic
 HDA Intel PCH Headphone
 HDA Intel PCH HDMI/DP,pcm		: 3=
 Logitech M325
-Printers-
No printers found
-SCSI Disks-
ATA TOSHIBA MQ01ABD1
ATA ST9750420AS
Slimtype BD  E  DS4E1S

Operating System
----------------

-Version-
Kernel		: Linux 4.4.0-21-generic (x86_64)
Compiled		: #37-Ubuntu SMP Mon Apr 18 18:33:37 UTC 2016
C Library		: Unknown
Default C Compiler		: GNU C Compiler version 5.4.0 20160609 (Ubuntu 5.4.0-6ubuntu1~16.04.2) 
Distribution		: Linux Mint 18 Sarah
-Current Session-
Computer Name		: jp-N73SV
User Name		: jp (jp)
Home Directory		: /home/jp
Desktop Environment		: X-Cinnamon (cinnamon)
-Misc-
Uptime		: 11 hours, 38 minutes
Load Average		: 0,00, 0,00, 0,00

Kernel Modules
--------------

-Loaded Modules-
hid_generic		: HID generic driver
drbg		: NIST SP800-90A Deterministic Random Bit Generator (DRBG) using following cores: HASH HMAC CTR
ansi_cprng		: Software Pseudo Random Number Generator
ctr		: CTR Counter block mode
ccm		: Counter with CBC MAC
bnep		: Bluetooth BNEP ver 1.3
binfmt_misc
snd_hda_codec_hdmi		: HDMI HD-audio codec
intel_rapl		: Driver for Intel RAPL (Running Average Power Limit)
x86_pkg_temp_thermal		: X86 PKG TEMP Thermal Driver
arc4		: ARC4 Cipher Algorithm
snd_hda_codec_realtek		: Realtek HD-audio codec
snd_hda_codec_generic		: Generic HD-audio codec parser
intel_powerclamp		: Package Level C-state Idle Injection for Intel CPUs
asus_nb_wmi		: Asus Notebooks WMI Hotkey Driver
coretemp		: Intel Core temperature monitor
asus_wmi		: Asus Generic WMI Driver
iwldvm		: Intel(R) Wireless WiFi Link AGN driver for Linux
sparse_keymap		: Generic support for sparse keymaps
snd_hda_intel		: Intel HDA driver
kvm_intel
snd_hda_codec		: HDA codec core
mac80211		: IEEE 802.11 subsystem
snd_hda_core		: HD-audio bus
kvm
uvcvideo		: USB Video Class driver
snd_hwdep		: Hardware dependent layer
irqbypass		: IRQ bypass manager utility module
videobuf2_vmalloc		: vmalloc memory handling routines for videobuf2
snd_pcm		: Midlevel PCM code for ALSA.
videobuf2_memops		: common memory handling routines for videobuf2
btusb		: Generic Bluetooth USB driver ver 0.8
videobuf2_v4l2		: Driver helper framework for Video for Linux 2
crct10dif_pclmul		: T10 DIF CRC calculation accelerated with PCLMULQDQ.
btrtl		: Bluetooth support for Realtek devices ver 0.1
videobuf2_core		: Driver helper framework for Video for Linux 2
snd_seq_midi		: Advanced Linux Sound Architecture sequencer MIDI synth.
iwlwifi		: Intel(R) Wireless WiFi driver for Linux
btbcm		: Bluetooth support for Broadcom devices ver 0.1
v4l2_common		: misc helper functions for v4l2 device drivers
crc32_pclmul
btintel		: Bluetooth support for Intel devices ver 0.1
videodev		: Device registrar for Video4Linux drivers v2
snd_seq_midi_event		: MIDI byte &lt;-&gt; sequencer event coder
bluetooth		: Bluetooth Core ver 2.21
aesni_intel		: Rijndael (AES) Cipher Algorithm, Intel AES-NI instructions optimized
media		: Device node registration for media drivers
aes_x86_64		: Rijndael (AES) Cipher Algorithm, asm optimized
lrw		: LRW block cipher mode
snd_rawmidi		: Midlevel RawMidi code for ALSA.
gf128mul		: Functions for multiplying elements of GF(2^128)
glue_helper
snd_seq		: Advanced Linux Sound Architecture sequencer.
ablk_helper
cfg80211		: wireless configuration support
cryptd		: Software async crypto daemon
input_leds		: Input -&gt; LEDs Bridge
joydev		: Joystick device interfaces
snd_seq_device		: ALSA sequencer device management
snd_timer		: ALSA timer interface
serio_raw		: Raw serio driver
snd		: Advanced Linux Sound Architecture driver for soundcards.
mei_me		: Intel(R) Management Engine Interface
soundcore		: Core sound module
mei		: Intel(R) Management Engine Interface
shpchp		: Standard Hot Plug PCI Controller Driver
lpc_ich		: LPC interface for Intel ICH
mac_hid
parport_pc		: PC-style parallel port driver
ppdev
lp
parport
autofs4
btrfs
xor
raid6_pq		: RAID6 Q-syndrome calculations
dm_mirror		: device-mapper mirror target
dm_region_hash		: device-mapper region hash
dm_log		: device-mapper dirty region log
hid_logitech_hidpp
hid_logitech_dj
usbhid		: USB HID core driver
hid
psmouse		: PS/2 mouse driver
nouveau		: nVidia Riva/TNT/GeForce/Quadro/Tesla
i915		: Intel Graphics
mxm_wmi		: MXM WMI Driver
ttm		: TTM memory manager subsystem (for DRM device)
i2c_algo_bit		: I2C-Bus bit-banging algorithm
drm_kms_helper		: DRM KMS helper
syscopyarea		: Generic copyarea (sys-to-sys)
sysfillrect		: Generic fill rectangle (sys-to-sys)
sysimgblt		: 1-bit/8-bit to 1-32 bit color expansion (sys-to-sys)
fb_sys_fops		: Generic file read (fb in system RAM)
ahci		: AHCI SATA low-level driver
drm		: DRM shared core routines
libahci		: Common AHCI SATA low-level routines
atl1c		: Qualcomm Atheros 100/1000M Ethernet Network Driver
wmi		: ACPI-WMI Mapping Driver
video		: ACPI Video Driver
fjes		: FUJITSU Extended Socket Network Device Driver

Boots
-----

-Boots-
Sat Aug 27 10:24		: 44..4.0-21-generic|still
Sat Aug 27 09:32		: 44..4.0-21-generic|-
Sat Aug 27 08:53		: 44..4.0-21-generic|-
Fri Aug 26 21:07		: 44..4.0-21-generic|-
Fri Aug 26 17:24		: 44..4.0-21-generic|-
Fri Aug 26 08:28		: 44..4.0-21-generic|-
Thu Aug 25 14:43		: 44..4.0-21-generic|-

Languages
---------

-Available Languages-
en_AG		: English language locale for Antigua and Barbuda
en_AG.utf8		: English language locale for Antigua and Barbuda
en_AU.utf8		: English locale for Australia
en_BW.utf8		: English locale for Botswana
en_CA.utf8		: English locale for Canada
en_DK.utf8		: English locale for Denmark
en_GB.utf8		: English locale for Britain
en_HK.utf8		: English locale for Hong Kong
en_IE.utf8		: English locale for Ireland
en_IN		: English language locale for India
en_IN.utf8		: English language locale for India
en_NG		: English locale for Nigeria
en_NG.utf8		: English locale for Nigeria
en_NZ.utf8		: English locale for New Zealand
en_PH.utf8		: English language locale for Philippines
en_SG.utf8		: English language locale for Singapore
en_US.utf8		: English locale for the USA
en_ZA.utf8		: English locale for South Africa
en_ZM		: English locale for Zambia
en_ZM.utf8		: English locale for Zambia
en_ZW.utf8		: English locale for Zimbabwe
fr_BE.utf8		: French locale for Belgium
fr_CA.utf8		: French locale for Canada
fr_CH.utf8		: French locale for Switzerland
fr_FR.utf8		: French locale for France
fr_LU.utf8		: French locale for Luxemburg

Filesystems
-----------

-Mounted File Systems-
udev	/dev	0,00 % (2,8 GiB of 2,8 GiB)	
tmpfs	/run	1,48 % (579,0 MiB of 587,7 MiB)	
/dev/sda1	/	50,91 % (8,9 GiB of 18,2 GiB)	
tmpfs	/dev/shm	0,09 % (2,9 GiB of 2,9 GiB)	
tmpfs	/run/lock	0,08 % (5,0 MiB of 5,0 MiB)	
tmpfs	/sys/fs/cgroup	0,00 % (2,9 GiB of 2,9 GiB)	
/dev/sda6	/home	73,00 % (241,6 GiB of 894,7 GiB)	
cgmfs	/run/cgmanager/fs	0,00 % (100,0 KiB of 100,0 KiB)	
tmpfs	/run/user/1000	0,01 % (587,6 MiB of 587,7 MiB)	

Display
-------

-Display-
Resolution		: 2944x1080 pixels
Vendor		: The X.Org Foundation
Version		: 1.18.3
-Monitors-
Monitor 0		: 1920x1080 pixels
Monitor 1		: 1024x768 pixels
-Extensions-
BIG-REQUESTS
Composite
DAMAGE
DOUBLE-BUFFER
DPMS
DRI2
GLX
Generic Event Extension
MIT-SCREEN-SAVER
MIT-SHM
Present
RANDR
RECORD
RENDER
SECURITY
SGI-GLX
SHAPE
SYNC
X-Resource
XC-MISC
XFIXES
XFree86-DGA
XFree86-VidModeExtension
XINERAMA
XInputExtension
XKEYBOARD
XTEST
XVideo
-OpenGL-
Vendor		: Intel Open Source Technology Center
Renderer		: Mesa DRI Intel(R) Sandybridge Mobile 
Version		: 3.0 Mesa 11.2.0
Direct Rendering		: Yes

Environment Variables
---------------------

-Environment Variables-
USER		: jp
LC_TIME		: fr_FR.UTF-8
XDG_SEAT		: seat0
SSH_AGENT_PID		: 1382
HOME		: /home/jp
MDM_LANG		: fr_FR.UTF-8
XDG_SESSION_COOKIE		: 2a5d5f96ef9147c0b35535562b32d0ff-1472286249.267460-1635956423
DESKTOP_SESSION		: cinnamon
GTK_MODULES		: gail:atk-bridge
QT_LINUX_ACCESSIBILITY_ALWAYS_ON		: 1
LC_MONETARY		: fr_FR.UTF-8
GDM_XSERVER_LOCATION		: local
DBUS_SESSION_BUS_ADDRESS		: unix:abstract=/tmp/dbus-qHHQe1U65s,guid=747acba10143167d27d2713a57c14e29
MDMSESSION		: cinnamon
MANDATORY_PATH		: /usr/share/gconf/cinnamon.mandatory.path
LOGNAME		: jp
DEFAULTS_PATH		: /usr/share/gconf/cinnamon.default.path
USERNAME		: jp
XDG_SESSION_ID		: c1
WINDOWPATH		: 8
PATH		: /usr/local/sbin:/usr/local/bin:/usr/sbin:/usr/bin:/sbin:/bin:/usr/games:/usr/local/games
PAPERSIZE		: a4
XDG_RUNTIME_DIR		: /run/user/1000
LC_ADDRESS		: fr_FR.UTF-8
DISPLAY		: :0
LANG		: fr_FR.UTF-8
LC_TELEPHONE		: fr_FR.UTF-8
XAUTHORITY		: /home/jp/.Xauthority
XDG_SESSION_DESKTOP		: cinnamon
SSH_AUTH_SOCK		: /run/user/1000/keyring/ssh
SHELL		: /bin/bash
LC_NAME		: fr_FR.UTF-8
GDMSESSION		: cinnamon
QT_ACCESSIBILITY		: 1
LC_MEASUREMENT		: fr_FR.UTF-8
LC_IDENTIFICATION		: fr_FR.UTF-8
XDG_VTNR		: 8
PWD		: /home/jp
XDG_DATA_DIRS		: /usr/share/cinnamon:/usr/share/gnome:/usr/local/share/:/usr/share/:/usr/share/mdm/
XDG_CONFIG_DIRS		: /etc/xdg/xdg-cinnamon:/etc/xdg
MDM_XSERVER_LOCATION		: local
LC_NUMERIC		: fr_FR.UTF-8
LC_PAPER		: fr_FR.UTF-8
GNOME_DESKTOP_SESSION_ID		: this-is-deprecated
QT_STYLE_OVERRIDE		: gtk
GTK_OVERLAY_SCROLLING		: 1
SESSION_MANAGER		: local/jp-N73SV:@/tmp/.ICE-unix/1315,unix/jp-N73SV:/tmp/.ICE-unix/1315
XDG_CURRENT_DESKTOP		: X-Cinnamon
GJS_DEBUG_OUTPUT		: stderr
GJS_DEBUG_TOPICS		: JS ERROR;JS LOG
CINNAMON_VERSION		: 3.0.6
GIO_LAUNCHED_DESKTOP_FILE		: /usr/share/applications/hardinfo.desktop
GIO_LAUNCHED_DESKTOP_FILE_PID		: 29444

Users
-----

-Users-
root		: root
daemon		: daemon
bin		: bin
sys		: sys
sync		: sync
games		: games
man		: man
lp		: lp
mail		: mail
news		: news
uucp		: uucp
proxy		: proxy
www-data		: www-data
backup		: backup
list		: Mailing List Manager
irc		: ircd
gnats		: Gnats Bug-Reporting System (admin)
nobody		: nobody
systemd-timesync		: systemd Time Synchronization
systemd-network		: systemd Network Management
systemd-resolve		: systemd Resolver
systemd-bus-proxy		: systemd Bus Proxy
syslog
_apt
messagebus
uuidd
ntp
avahi-autoipd		: Avahi autoip daemon
avahi		: Avahi mDNS daemon
dnsmasq		: dnsmasq
colord		: colord colour management daemon
speech-dispatcher		: Speech Dispatcher
hplip		: HPLIP system user
kernoops		: Kernel Oops Tracking Daemon
pulse		: PulseAudio daemon
nm-openvpn		: NetworkManager OpenVPN
rtkit		: RealtimeKit
saned
usbmux		: usbmux daemon
mdm		: MDM Display Manager
jp		: jp
clamav

Devices
*******


Processor
---------

-Processors-
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2600,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2600,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2622,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2600,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2599,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2600,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2643,00MHz
Intel(R) Core(TM) i7-2630QM CPU @ 2.00GHz		: 2596,00MHz

Memory
------

-Memory-
Total Memory		: 6017808 kB
Free Memory		: 496372 kB
MemAvailable		: 3906740 kB
Buffers		: 642132 kB
Cached		: 2158644 kB
Cached Swap		: 3056 kB
Active		: 2312772 kB
Inactive		: 1924544 kB
Active(anon)		: 1118484 kB
Inactive(anon)		: 825292 kB
Active(file)		: 1194288 kB
Inactive(file)		: 1099252 kB
Unevictable		: 20 kB
Mlocked		: 20 kB
Virtual Memory		: 3998716 kB
Free Virtual Memory		: 3966772 kB
Dirty		: 156 kB
Writeback		: 0 kB
AnonPages		: 1433972 kB
Mapped		: 404180 kB
Shmem		: 507228 kB
Slab		: 1203548 kB
SReclaimable		: 1153260 kB
SUnreclaim		: 50288 kB
KernelStack		: 8720 kB
PageTables		: 25192 kB
NFS_Unstable		: 0 kB
Bounce		: 0 kB
WritebackTmp		: 0 kB
CommitLimit		: 7007620 kB
Committed_AS		: 4795536 kB
VmallocTotal		: 34359738367 kB
VmallocUsed		: 0 kB
VmallocChunk		: 0 kB
HardwareCorrupted		: 0 kB
AnonHugePages		: 360448 kB
CmaTotal		: 0 kB
CmaFree		: 0 kB
HugePages_Total		: 0
HugePages_Free		: 0
HugePages_Rsvd		: 0
HugePages_Surp		: 0
Hugepagesize		: 2048 kB
DirectMap4k		: 148652 kB
DirectMap2M		: 6051840 kB

PCI Devices
-----------

-PCI Devices-
Host bridge		: Intel Corporation 2nd Generation Core Processor Family DRAM Controller (rev 09)
PCI bridge		: Intel Corporation Xeon E3-1200/2nd Generation Core Processor Family PCI Express Root Port (rev 09) (prog-if 00 [Normal decode])
VGA compatible controller		: Intel Corporation 2nd Generation Core Processor Family Integrated Graphics Controller (rev 09) (prog-if 00 [VGA controller])
Communication controller		: Intel Corporation 6 Series/C200 Series Chipset Family MEI Controller #1 (rev 04)
USB controller		: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #2 (rev 05) (prog-if 20 [EHCI])
Audio device		: Intel Corporation 6 Series/C200 Series Chipset Family High Definition Audio Controller (rev 05)
PCI bridge		: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 1 (rev b5) (prog-if 00 [Normal decode])
PCI bridge		: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 2 (rev b5) (prog-if 00 [Normal decode])
PCI bridge		: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 4 (rev b5) (prog-if 00 [Normal decode])
PCI bridge		: Intel Corporation 6 Series/C200 Series Chipset Family PCI Express Root Port 6 (rev b5) (prog-if 00 [Normal decode])
USB controller		: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #1 (rev 05) (prog-if 20 [EHCI])
ISA bridge		: Intel Corporation HM65 Express Chipset Family LPC Controller (rev 05)
SATA controller		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
SMBus		: Intel Corporation 6 Series/C200 Series Chipset Family SMBus Controller (rev 05)
VGA compatible controller		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
Multimedia controller		: Philips Semiconductors SAA7231 (rev ca)
Network controller		: Intel Corporation Centrino Wireless-N 1000 [Condor Peak]
USB controller		: Fresco Logic FL1000G USB 3.0 Host Controller (rev 04) (prog-if 30 [XHCI])
Ethernet controller		: Qualcomm Atheros AR8151 v2.0 Gigabit Ethernet (rev c0)

USB Devices
-----------


Printers
--------

-Printers-
No printers found

Battery
-------

-No batteries-
No batteries found on this system

Sensors
-------


Input Devices
-------------

-Input Devices-
 Lid Switch
 Sleep Button
 Power Button
 AT Translated Set 2 keyboard
 Video Bus
 Video Bus
 ETPS/2 Elantech Touchpad
 USB2.0 UVC 2M WebCam
 Asus WMI hotkeys
 HDA Intel PCH Mic
 HDA Intel PCH Headphone
 HDA Intel PCH HDMI/DP,pcm		: 3=
 Logitech M325

Storage
-------

-SCSI Disks-
ATA TOSHIBA MQ01ABD1
ATA ST9750420AS
Slimtype BD  E  DS4E1S

DMI
---

-BIOS-
Date		: 08/18/2011
Vendor		: American Megatrends Inc. (www.ami.com)
Version		: N73SV.306
-Board-
Name		: N73SV
Vendor		: ASUSTeK Computer Inc. (SEAGATE, www.seagate.com)

Resources
---------

-I/O Ports-
<tt>0000-0cf7 </tt>		: PCI Bus 0000:00
<tt>  0000-001f </tt>		: dma1
<tt>  0020-0021 </tt>		: pic1
<tt>  0040-0043 </tt>		: timer0
<tt>  0050-0053 </tt>		: timer1
<tt>  0060-0060 </tt>		: keyboard
<tt>  0062-0062 </tt>		: PNP0C09:00
<tt>    0062-0062 </tt>		: EC data
<tt>  0064-0064 </tt>		: keyboard
<tt>  0066-0066 </tt>		: PNP0C09:00
<tt>    0066-0066 </tt>		: EC cmd
<tt>  0070-0077 </tt>		: rtc0
<tt>  0080-008f </tt>		: dma page reg
<tt>  00a0-00a1 </tt>		: pic2
<tt>  00c0-00df </tt>		: dma2
<tt>  00f0-00ff </tt>		: fpu
<tt>    00f0-00f0 </tt>		: PNP0C04:00
<tt>  03c0-03df </tt>		: vesafb
<tt>  0400-0403 </tt>		: ACPI PM1a_EVT_BLK
<tt>  0404-0405 </tt>		: ACPI PM1a_CNT_BLK
<tt>  0408-040b </tt>		: ACPI PM_TMR
<tt>  0410-0415 </tt>		: ACPI CPU throttle
<tt>  0420-042f </tt>		: ACPI GPE0_BLK
<tt>  0430-0433 </tt>		: iTCO_wdt.0.auto
<tt>  0450-0450 </tt>		: ACPI PM2_CNT_BLK
<tt>  0454-0457 </tt>		: pnp 00:02
<tt>  0458-047f </tt>		: pnp 00:00
<tt>    0460-047f </tt>		: iTCO_wdt.0.auto
<tt>  0500-057f </tt>		: pnp 00:00
<tt>  0680-069f </tt>		: pnp 00:00
<tt>0cf8-0cff </tt>		: PCI conf1
<tt>0d00-ffff </tt>		: PCI Bus 0000:00
<tt>  1000-100f </tt>		: pnp 00:00
<tt>  164e-164f </tt>		: pnp 00:00
<tt>  9000-9fff </tt>		: PCI Bus 0000:05
<tt>    9000-907f </tt>		: Qualcomm Atheros AR8151 v2.0 Gigabit Ethernet (rev c0)
<tt>      9000-907f </tt>		: Qualcomm Atheros 100/1000M Ethernet Network Driver
<tt>  a000-afff </tt>		: PCI Bus 0000:04
<tt>  b000-bfff </tt>		: PCI Bus 0000:03
<tt>  c000-cfff </tt>		: PCI Bus 0000:02
<tt>  d000-dfff </tt>		: PCI Bus 0000:01
<tt>    d000-d07f </tt>		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
<tt>  e000-e03f </tt>		: Intel Corporation 2nd Generation Core Processor Family Integrated Graphics Controller (rev 09) (prog-if 00 [VGA controller])
<tt>  e040-e05f </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family SMBus Controller (rev 05)
<tt>  e060-e07f </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    e060-e07f </tt>		: AHCI SATA low-level driver
<tt>  e080-e083 </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    e080-e083 </tt>		: AHCI SATA low-level driver
<tt>  e090-e097 </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    e090-e097 </tt>		: AHCI SATA low-level driver
<tt>  e0a0-e0a3 </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    e0a0-e0a3 </tt>		: AHCI SATA low-level driver
<tt>  e0b0-e0b7 </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    e0b0-e0b7 </tt>		: AHCI SATA low-level driver
<tt>  ffff-ffff </tt>		: pnp 00:00
<tt>    ffff-ffff </tt>		: pnp 00:00
-Memory-
<tt>00000000-00000fff </tt>		: reserved
<tt>00001000-0009e7ff </tt>		: System RAM
<tt>0009e800-0009ffff </tt>		: reserved
<tt>000a0000-000bffff </tt>		: PCI Bus 0000:00
<tt>000c0000-000cedff </tt>		: Video ROM
<tt>000d0000-000d3fff </tt>		: PCI Bus 0000:00
<tt>000d4000-000d7fff </tt>		: PCI Bus 0000:00
<tt>000d8000-000dbfff </tt>		: PCI Bus 0000:00
<tt>000dc000-000dffff </tt>		: PCI Bus 0000:00
<tt>000e0000-000fffff </tt>		: reserved
<tt>  000e0000-000e3fff </tt>		: PCI Bus 0000:00
<tt>  000e4000-000e7fff </tt>		: PCI Bus 0000:00
<tt>  000f0000-000fffff </tt>		: System ROM
<tt>00100000-1fffffff </tt>		: System RAM
<tt>  01000000-01829385 </tt>		: Kernel code
<tt>  01829386-01f3f93f </tt>		: Kernel data
<tt>  020ba000-021fcfff </tt>		: Kernel bss
<tt>20000000-201fffff </tt>		: reserved
<tt>  20000000-201fffff </tt>		: pnp 00:07
<tt>20200000-3fffffff </tt>		: System RAM
<tt>40000000-401fffff </tt>		: reserved
<tt>  40000000-401fffff </tt>		: pnp 00:07
<tt>40200000-aabd1fff </tt>		: System RAM
<tt>aabd2000-aacf8fff </tt>		: reserved
<tt>aacf9000-aacfafff </tt>		: System RAM
<tt>aacfb000-aad8dfff </tt>		: reserved
<tt>aad8e000-aad8efff </tt>		: System RAM
<tt>aad8f000-aadb7fff </tt>		: reserved
<tt>aadb8000-aadc7fff </tt>		: System RAM
<tt>aadc8000-aade7fff </tt>		: reserved
<tt>aade8000-aaf18fff </tt>		: System RAM
<tt>aaf19000-aafe7fff </tt>		: ACPI Non-volatile Storage
<tt>aafe8000-aaffcfff </tt>		: System RAM
<tt>aaffd000-aaffffff </tt>		: ACPI Tables
<tt>ab000000-af9fffff </tt>		: reserved
<tt>  aba00000-af9fffff </tt>		: Graphics Stolen Memory
<tt>afa00000-feafffff </tt>		: PCI Bus 0000:00
<tt>  afa00000-afa00fff </tt>		: pnp 00:05
<tt>    afa00000-afa00fff </tt>		: pnp 00:06
<tt>  b0000000-bfffffff </tt>		: Intel Corporation 2nd Generation Core Processor Family Integrated Graphics Controller (rev 09) (prog-if 00 [VGA controller])
<tt>  c0000000-d1ffffff </tt>		: PCI Bus 0000:01
<tt>    c0000000-cfffffff </tt>		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
<tt>    d0000000-d1ffffff </tt>		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
<tt>  d2100000-d2afffff </tt>		: PCI Bus 0000:05
<tt>  d2c00000-d35fffff </tt>		: PCI Bus 0000:04
<tt>  d3700000-d40fffff </tt>		: PCI Bus 0000:03
<tt>  d4200000-d4bfffff </tt>		: PCI Bus 0000:02
<tt>  db000000-dc0fffff </tt>		: PCI Bus 0000:01
<tt>    db000000-dbffffff </tt>		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
<tt>    dc000000-dc07ffff </tt>		: NVIDIA Corporation GF108M [GeForce GT 540M] (rev a1) (prog-if 00 [VGA controller])
<tt>  dc400000-dc7fffff </tt>		: Intel Corporation 2nd Generation Core Processor Family Integrated Graphics Controller (rev 09) (prog-if 00 [VGA controller])
<tt>  dc800000-dd1fffff </tt>		: PCI Bus 0000:02
<tt>    dc800000-dcbfffff </tt>		: Philips Semiconductors SAA7231 (rev ca)
<tt>    dcc00000-dcffffff </tt>		: Philips Semiconductors SAA7231 (rev ca)
<tt>  dd300000-ddcfffff </tt>		: PCI Bus 0000:05
<tt>    dd300000-dd33ffff </tt>		: Qualcomm Atheros AR8151 v2.0 Gigabit Ethernet (rev c0)
<tt>      dd300000-dd33ffff </tt>		: Qualcomm Atheros 100/1000M Ethernet Network Driver
<tt>  ddd00000-de6fffff </tt>		: PCI Bus 0000:04
<tt>    ddd00000-ddd0ffff </tt>		: Fresco Logic FL1000G USB 3.0 Host Controller (rev 04) (prog-if 30 [XHCI])
<tt>      ddd00000-ddd0ffff </tt>		: xhci-hcd
<tt>  de700000-df0fffff </tt>		: PCI Bus 0000:03
<tt>    de700000-de701fff </tt>		: Intel Corporation Centrino Wireless-N 1000 [Condor Peak]
<tt>      de700000-de701fff </tt>		: Intel(R) Wireless WiFi driver for Linux
<tt>  df100000-df103fff </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family High Definition Audio Controller (rev 05)
<tt>    df100000-df103fff </tt>		: ICH HD audio
<tt>  df105000-df1050ff </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family SMBus Controller (rev 05)
<tt>  df106000-df1067ff </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family 6 port SATA AHCI Controller (rev 05) (prog-if 01 [AHCI 1.0])
<tt>    df106000-df1067ff </tt>		: AHCI SATA low-level driver
<tt>  df107000-df1073ff </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #1 (rev 05) (prog-if 20 [EHCI])
<tt>    df107000-df1073ff </tt>		: ehci_hcd
<tt>  df108000-df1083ff </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family USB Enhanced Host Controller #2 (rev 05) (prog-if 20 [EHCI])
<tt>    df108000-df1083ff </tt>		: ehci_hcd
<tt>  df10a000-df10a00f </tt>		: Intel Corporation 6 Series/C200 Series Chipset Family MEI Controller #1 (rev 04)
<tt>    df10a000-df10a00f </tt>		: Intel(R) Management Engine Interface
<tt>  e0000000-e3ffffff </tt>		: PCI MMCONFIG 0000 [bus 00-3f]
<tt>    e0000000-e3ffffff </tt>		: reserved
<tt>      e0000000-e3ffffff </tt>		: pnp 00:05
<tt>fec00000-fec00fff </tt>		: reserved
<tt>  fec00000-fec003ff </tt>		: IOAPIC 0
<tt>fed00000-fed003ff </tt>		: HPET 0
<tt>  fed00000-fed003ff </tt>		: PNP0103:00
<tt>fed10000-fed13fff </tt>		: reserved
<tt>fed18000-fed19fff </tt>		: reserved
<tt>  fed18000-fed18fff </tt>		: pnp 00:05
<tt>  fed19000-fed19fff </tt>		: pnp 00:05
<tt>fed1c000-fed1ffff </tt>		: reserved
<tt>  fed1c000-fed1ffff </tt>		: pnp 00:05
<tt>    fed1f410-fed1f414 </tt>		: iTCO_wdt.0.auto
<tt>fed20000-fed3ffff </tt>		: pnp 00:05
<tt>fed40000-fed44fff </tt>		: PCI Bus 0000:00
<tt>fed45000-fed8ffff </tt>		: pnp 00:05
<tt>fed90000-fed93fff </tt>		: pnp 00:05
<tt>fee00000-fee00fff </tt>		: Local APIC
<tt>  fee00000-fee00fff </tt>		: reserved
<tt>ff000000-ffffffff </tt>		: INT0800:00
<tt>  ff980000-ffbfffff </tt>		: reserved
<tt>  ffd80000-ffffffff </tt>		: reserved
<tt>100000000-1cfdfffff </tt>		: System RAM
<tt>1cfe00000-1cfffffff </tt>		: RAM buffer
-DMA-
<tt> 4</tt>		: cascade

Network
*******


Interfaces
----------

-Network Interfaces-
enp5s0	0,00MiB	0,00MiB		
lo	1,28MiB	1,28MiB	127.0.0.1	
wlp3s0	962,58MiB	77,22MiB	192.168.1.94	

IP Connections
--------------

-Connections-
127.0.1.1:53		0.0.0.0:*	udp	
127.0.0.1:631	LISTEN	0.0.0.0:*	tcp	
192.168.1.94:57046	ESTABLISHED	188.125.69.5:993	tcp	
192.168.1.94:43478	ESTABLISHED	64.233.167.190:443	tcp	
192.168.1.94:40878	LAST_ACK	188.125.69.6:993	tcp	
192.168.1.94:46196	ESTABLISHED	74.125.133.95:443	tcp	
192.168.1.94:57796	ESTABLISHED	66.102.1.108:993	tcp	
192.168.1.94:41096	ESTABLISHED	54.165.177.196:443	tcp	
192.168.1.94:50728	ESTABLISHED	194.117.213.11:993	tcp	
192.168.1.94:35220	ESTABLISHED	74.125.71.109:993	tcp	
192.168.1.94:35218	ESTABLISHED	74.125.71.109:993	tcp	
192.168.1.94:57066	ESTABLISHED	188.125.69.5:993	tcp	
192.168.1.94:41094	ESTABLISHED	54.165.177.196:443	tcp	
192.168.1.94:53004	LAST_ACK	188.125.69.63:993	tcp	
192.168.1.94:57804	ESTABLISHED	66.102.1.108:993	tcp	
::1:631	LISTEN	:::*	tcp6	
0.0.0.0:5353		0.0.0.0:*	udp	
0.0.0.0:48270		0.0.0.0:*	udp	
0.0.0.0:36115		0.0.0.0:*	udp	
127.0.1.1:53		0.0.0.0:*	udp	
0.0.0.0:68		0.0.0.0:*	udp	
192.168.1.94:123		0.0.0.0:*	udp	
127.0.0.1:123		0.0.0.0:*	udp	
0.0.0.0:123		0.0.0.0:*	udp	
0.0.0.0:631		0.0.0.0:*	udp	
:::5353		:::*	udp6	
:::35735		:::*	udp6	
:::60655		:::*	udp6	
fe80::4241:a968:4c3:123		:::*	udp6	
::1:123		:::*	udp6	
:::123		:::*	udp6	

Routing Table
-------------

-IP routing table-
0.0.0.0 / 192.168.1.1	0.0.0.0	UG	wlp3s0	
169.254.0.0 / 0.0.0.0	255.255.0.0	U	wlp3s0	
192.168.1.0 / 0.0.0.0	255.255.255.0	U	wlp3s0	

ARP Table
---------

-ARP Table-
192.168.1.17	00:00:00:00:00:00	wlp3s0	
192.168.1.39	00:00:00:00:00:00	wlp3s0	
192.168.1.99	00:26:37:f4:5a:e9	wlp3s0	
192.168.1.1	00:25:15:a8:da:48	wlp3s0	
192.168.1.77	00:00:00:00:00:00	wlp3s0	
192.168.1.82	00:00:00:00:00:00	wlp3s0	
192.168.1.53	b0:df:3a:d6:d8:6a	wlp3s0	
192.168.1.6	00:00:00:00:00:00	wlp3s0	
192.168.1.7	00:00:00:00:00:00	wlp3s0	
192.168.1.21	00:00:00:00:00:00	wlp3s0	
192.168.1.103	00:00:00:00:00:00	wlp3s0	
192.168.1.5	00:00:00:00:00:00	wlp3s0	
192.168.1.26	00:00:00:00:00:00	wlp3s0	
192.168.1.70	00:00:00:00:00:00	wlp3s0	
192.168.1.27	98:52:b1:3c:4c:c7	wlp3s0	
192.168.1.40	00:00:00:00:00:00	wlp3s0	
192.168.1.10	00:00:00:00:00:00	wlp3s0	
192.168.1.11	00:00:00:00:00:00	wlp3s0	
192.168.1.41	00:00:00:00:00:00	wlp3s0	
192.168.1.128	00:00:00:00:00:00	wlp3s0	
192.168.1.106	00:00:00:00:00:00	wlp3s0	
192.168.1.9	00:00:00:00:00:00	wlp3s0	
192.168.1.14	00:00:00:00:00:00	wlp3s0	
192.168.1.91	00:00:00:00:00:00	wlp3s0	
192.168.1.45	00:00:00:00:00:00	wlp3s0	
192.168.1.28	30:c7:ae:a6:b6:b1	wlp3s0	
192.168.1.15	00:00:00:00:00:00	wlp3s0	
192.168.1.75	00:00:00:00:00:00	wlp3s0	
192.168.1.29	00:00:00:00:00:00	wlp3s0	
192.168.1.127	00:00:00:00:00:00	wlp3s0	
192.168.1.34	00:00:00:00:00:00	wlp3s0	
192.168.1.12	00:00:00:00:00:00	wlp3s0	
192.168.1.13	00:00:00:00:00:00	wlp3s0	
192.168.1.18	00:00:00:00:00:00	wlp3s0	
192.168.1.49	00:00:00:00:00:00	wlp3s0	
192.168.1.3	00:00:00:00:00:00	wlp3s0	
192.168.1.16	00:00:00:00:00:00	wlp3s0	
192.168.1.54	00:00:00:00:00:00	wlp3s0	

DNS Servers
-----------

-Name servers-
127.0.1.1

Statistics
----------

-IP-
781595		: Total packets received
1		: With invalid addresses
0		: Incoming packets discarded
0		: Incoming packets discarded
775050		: Incoming packets delivered
537029		: Requests sent out
16		: Outgoing packets dropped
-ICMP-
418		: ICMP messages received
0		: ICMP messages failed
855		: ICMP messages sent
0		: ICMP messages failed
-ICMPMSG-
-TCP-
3449		: Active connections openings
22		: Passive connection openings
17		: Failed connection attempts
131		: Connection resets received
11		: Connections established
659831		: Segments received
429185		: Segments send out
1506		: Segments retransmited
45		: Bad segments received.
1861		: Resets sent
-UDP-
110254		: Packets received
3478		: Packets to unknown port received.
0		: Packet receive errors
105151		: Packets sent
-UDPLITE-
-TCPEXT-
7		: Packets pruned from receive queue because of socket buffer overrun
1024		: TCP sockets finished time wait in fast timer
6		: Packets header predicted and directly queued to user
4955		: Delayed acks sent
4		: Timeouts after SACK recovery
9		: Connections reset due to early user close
7813		: Bytes directly received in process context from prequeue
537833		: Packet headers predicted
6		: Packets header predicted and directly queued to user
13753		: Acknowledgments not containing data payload received
4800		: Predicted acknowledgments
64		: Times recovered from packet loss by selective acknowledgements
3		: Forward retransmits
167		: Congestion windows recovered without slow start after partial ack
4		: Timeouts after SACK recovery
224		: Fast retransmits
3		: Forward retransmits
262		: Other TCP timeouts
2		: DSACKs for out of order packets received
88		: Packets collapsed in receive queue due to low socket buffer
335		: DSACKs sent for old packets
19		: DSACKs sent for out of order packets
105		: DSACKs received
2		: DSACKs for out of order packets received
363		: Connections reset due to unexpected data
9		: Connections reset due to early user close
75		: Connections aborted due to timeout
-IPEXT-

Shared Directories
------------------

-SAMBA-
-NFS-

Benchmarks
**********


CPU Blowfish
------------

-CPU Blowfish-
<big><b>This Machine</b></big>	2600 MHz	2,434	
Intel(R) Celeron(R) M processor         1.50GHz	(null)	26.1876862	
PowerPC 740/750 (280.00MHz)	(null)	172.816713	

CPU CryptoHash
--------------

-CPU CryptoHash-
<big><b>This Machine</b></big>	2600 MHz	593,677	

CPU Fibonacci
-------------

-CPU Fibonacci-
<big><b>This Machine</b></big>	2600 MHz	1,890	
Intel(R) Celeron(R) M processor         1.50GHz	(null)	8.1375674	
PowerPC 740/750 (280.00MHz)	(null)	58.07682	

CPU N-Queens
------------

-CPU N-Queens-
<big><b>This Machine</b></big>	2600 MHz	0,592	

FPU FFT
-------

-FPU FFT-
<big><b>This Machine</b></big>	2600 MHz	1,189	

FPU Raytracing
--------------

-FPU Raytracing-
<big><b>This Machine</b></big>	2600 MHz	3,792	
Intel(R) Celeron(R) M processor         1.50GHz	(null)	40.8816714	
PowerPC 740/750 (280.00MHz)	(null)	161.312647	
